{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"merged":[[0,0,0,6],[1,0,1,6],[12,0,12,6],[15,0,15,6],[38,0,38,6],[40,0,40,6],[41,6,43,6]],"flags":["formulas_cached_only"]}
["2023年12月采购计划补充标段"]
["标段1化轻杂品类"]
[1,"消防器材架",null,"36.5长*29.5高*19.5宽 工程塑料材质","个",30]
[2,"灭火器","淮海","8kg","瓶",10]
[3,"消防带","淮海","φ50","盘",10,"带快接"]
[4,"消防水枪","淮海","二寸","支",3,"含接头"]
[5,"消防栓快接头（带内丝）","淮海","φ50","只",20]
[6,"透明气管",null,"12mm","米",100]
[7,"聚四氟乙烯管",null,"12mm","米",60]
[8,"红地毯浴室防滑垫",null,"PVC-1.2米宽5mm厚","米",45]
[9,"防冻液","长城","-45°   20L/桶","桶",5]
[10,"通风带",null,"φ500阻燃  10米/根  正压","根",50,"必须带安标证"]
["标段2高筒靴类"]
[1,"高筒胶靴","飞鹤","40-43码","双",600,"40码80双 41码120双 42码43码各200双"]
[2,"高筒胶靴","飞鹤","45-46","双",80,"45码46码各40双"]
["标段3机电杂品类"]
[1,"电接点压力表","红旗","0-60MPa 380V 30VA","件",2]
[2,"光电开关","施耐德","XUX5ARCNT16 ","件",2]
[3,"单向阀","SMC","AK4000-04","只",2]
[4,"调压过滤器","SMC","AW40-04D-B 0.05-0.85MPa","只",2]
[5,"常开电磁阀","宜工","2K250-25 DN20 AC220V","只",2]
[6,"丝攻","上工","M20","副",5]
[7,"丝攻","上工","M18","副",5]
[8,"丝攻","上工","M16","副",5]
[9,"切割片","东成","400MM","片",50]
[10,"切割片","东成","100MM","片",400]
[11,"OT接线鼻子","凤凰","100A","个",200]
[12,"D104石墨碳刷","摩根","25*32*60","件",50]
[13,"poe摄像头","海康威视","海康威视","台",5]
[14,"压力表","上海天川","0-6MPa  直径150mm ","支",20]
[15,"负压表","上海天川","-0.1-1.6MPa","支",10]
[16,"压力表","红旗","0-0.6MPa  直径100mm","个",6]
[17,"氧气表","得力",null,"块",10]
[18,"丙烷表","得力",null,"块",10]
[19,"电接点隔膜压力表","大成","0-40MPa 直径150mm","件",1]
[20,"高压10kv冷缩终端接头","万博","20-50平方 户外","套",20]
[21,"磁感应开关","洛阳原创","KGE1-1AP","只",15]
[22,"数字式温度显示调节仪","大连世有","XMT-22B","台",2]
["标段4铲运机电缆类"]
[1,"铲运机专用电缆","拓柔","3*16+1*10","米",500,"低烟无卤阻燃,必须带矿安\n"]
["标段5商砼类"]
[1,"商砼",null,"C30","方",1500,"含泵送费，要求正规搅拌站（所有资质齐全）接受第三方检验结果。送货地点：吴庄选矿厂 分批次送货。此报价单单价为不含增值税价格。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}